REM This is BadUSB demo script for Chrome and ChromeOS by kowalski7cc

REM Exit from Overview
ESC
REM Open a new tab
CTRL t
REM wait for some slower chromebooks
DELAY 1000
REM Make sure we have omnibox focus
CTRL l
DELAY 200
REM Open an empty editable page
DEFAULT_DELAY 50
STRING data:text/html, <html contenteditable autofocus><title>Flipper Zero BadUSB Demo</title><style>body{font-family:monospace;}
ENTER
DELAY 500

STRING Hello World!
ENTER

REM Copy-Paste previous string
UP
HOME
SHIFT DOWN
CTRL c
RIGHT
CTRL v
CTRL v


STRING =
REPEAT 59
ENTER
ENTER

STRING               _.-------.._                    -,
ENTER
HOME
STRING           .-"```"--..,,_/ /`-,               -,  \ 
ENTER
HOME
STRING        .:"          /:/  /'\  \     ,_...,  `. |  |
ENTER
HOME
STRING       /       ,----/:/  /`\ _\~`_-"`     _;
ENTER
HOME
STRING      '      / /`"""'\ \ \.~`_-'      ,-"'/ 
ENTER
HOME
STRING     |      | |  0    | | .-'      ,/`  /
ENTER
HOME
STRING    |    ,..\ \     ,.-"`       ,/`    /
ENTER
HOME
STRING   ;    :    `/`""\`           ,/--==,/-----,
ENTER
HOME
STRING   |    `-...|        -.___-Z:_______J...---;
ENTER
HOME
STRING   :         `                           _-'
ENTER
HOME
STRING  _L_  _     ___  ___  ___  ___  ____--"`
ENTER
HOME
STRING | __|| |   |_ _|| _ \| _ \| __|| _ \ 
ENTER
HOME
STRING | _| | |__  | | |  _/|  _/| _| |   / 
ENTER
HOME
STRING |_|  |____||___||_|  |_|  |___||_|_\ 
ENTER
HOME
ENTER

STRING Flipper Zero BadUSB feature is compatible with USB Rubber Ducky script format
ENTER
STRING More information about script syntax can be found here:
ENTER
STRING https://github.com/flipperdevices/flipperzero-firmware/blob/dev/documentation/file_formats/BadUsbScriptFormat.md
ENTER
