ID 1234:5678 Apple:Keyboard
REM You can change these values to VID/PID of original Apple keyboard
REM to bypass Keyboard Setup Assistant

REM This is BadUSB demo script for macOS

REM Open terminal window
DELAY 1000
GUI SPACE
DELAY 500
STRING terminal
DELAY 500
ENTER
DELAY 750

REM Copy-Paste previous string
UP
CTRL c

REM Bigger shell script example
STRING cat > /dev/null << EOF
ENTER

STRING Hello World!
ENTER

DEFAULT_DELAY 50

STRING =
REPEAT 59
ENTER
ENTER

STRING               _.-------.._                    -,
ENTER
HOME
STRING           .-"'''"--..,,_/ /'-,               -,  \
ENTER
HOME
STRING        .:"          /:/  /'\  \     ,_...,  '. |  |
ENTER
HOME
STRING       /       ,----/:/  /'\ _\~'_-"'     _;
ENTER
HOME
STRING      '      / /'"""'\ \ \.~'_-'      ,-"'/
ENTER
HOME
STRING     |      | |  0    | | .-'      ,/'  /
ENTER
HOME
STRING    |    ,..\ \     ,.-"'       ,/'    /
ENTER
HOME
STRING   ;    :    '/'""\'           ,/--==,/-----,
ENTER
HOME
STRING   |    '-...|        -.___-Z:_______J...---;
ENTER
HOME
STRING   :         '                           _-'
ENTER
HOME
STRING  _L_  _     ___  ___  ___  ___  ____--"'
ENTER
HOME
STRING | __|| |   |_ _|| _ \| _ \| __|| _ \
ENTER
HOME
STRING | _| | |__  | | |  _/|  _/| _| |   /
ENTER
HOME
STRING |_|  |____||___||_|  |_|  |___||_|_\
ENTER
HOME
ENTER

STRING Flipper Zero BadUSB feature is compatible with USB Rubber Ducky script format
ENTER
STRING More information about script syntax can be found here:
ENTER
STRING https://github.com/flipperdevices/flipperzero-firmware/blob/dev/documentation/file_formats/BadUsbScriptFormat.md
ENTER

STRING EOF
ENTER
