00001524-1212-EFDE-1523-785FEABCD123  Blinky Button State  [char:nordic]
00001525-1212-EFDE-1523-785FEABCD123  Blinky LED State  [char:nordic]
00001531-1212-EFDE-1523-785FEABCD123  Legacy DFU Control Point  [char:nordic]
00001532-1212-EFDE-1523-785FEABCD123  Legacy DFU Packet  [char:nordic]
00001534-1212-EFDE-1523-785FEABCD123  Legacy DFU Version  [char:nordic]
00001624-1212-EFDE-1623-785FEABCD123  LEGO® Wireless Protocol v3 Hub Characteristic  [char:lego]
00001626-1212-EFDE-1623-785FEABCD123  LEGO® Wireless Protocol v3 Bootloader Characteristic  [char:lego]
0A852C59-50D3-4492-BFD3-22FE58A24F01  Helium Hotspot Public Key  [char:helium]
1233  Deprecated Fast Pair Model ID  [char:google]
1234  Deprecated Fast Pair Key-based Pairing  [char:google]
1235  Deprecated Fast Pair Passkey  [char:google]
1236  Deprecated Fast Pair Account Key  [char:google]
1237  Deprecated Fast Pair Data  [char:google]
14387801-130C-49E7-B877-2881C89CB258  Wi-Fi Provisioning Service Version  [char:nordic]
14387802-130C-49E7-B877-2881C89CB258  Wi-Fi Provisioning Control Point  [char:nordic]
14387803-130C-49E7-B877-2881C89CB258  Wi-Fi Provisioning Data Out  [char:nordic]
1524  Throughput Characteristic  [char:nordic]
180EFDEF-7579-4B4A-B2DF-72733B7FA2FE  Helium Hotspot Lights  [char:helium]
21490001-494A-4573-98AF-F126AF76F490  Distance Measurement Characteristic  [char:nordic]
21490002-494A-4573-98AF-F126AF76F490  Azimuth Measurement Characteristic  [char:nordic]
21490003-494A-4573-98AF-F126AF76F490  Elevation Measurement Characteristic  [char:nordic]
21490004-494A-4573-98AF-F126AF76F490  DDF Feature  [char:nordic]
21490005-494A-4573-98AF-F126AF76F490  Control Point  [char:nordic]
22EAC6E9-24D6-4BB5-BE44-B36ACE7C7BFB  Apple Data Source  [char:apple]
2A00  Device Name  [char:gss]
2A01  Appearance  [char:gss]
2A02  Peripheral Privacy Flag  [char:gss]
2A03  Reconnection Address  [char:gss]
2A04  Peripheral Preferred Connection Parameters  [char:gss]
2A05  Service Changed  [char:gss]
2A06  Alert Level  [char:gss]
2A07  Tx Power Level  [char:gss]
2A08  Date Time  [char:gss]
2A09  Day of Week  [char:gss]
2A0A  Day Date Time  [char:gss]
2A0B  Exact Time 100  [char:gss]
2A0C  Exact Time 256  [char:gss]
2A0D  DST Offset  [char:gss]
2A0E  Time Zone  [char:gss]
2A0F  Local Time Information  [char:gss]
2A10  Secondary Time Zone  [char:gss]
2A11  Time with DST  [char:gss]
2A12  Time Accuracy  [char:gss]
2A13  Time Source  [char:gss]
2A14  Reference Time Information  [char:gss]
2A15  Time Broadcast  [char:gss]
2A16  Time Update Control Point  [char:gss]
2A17  Time Update State  [char:gss]
2A18  Glucose Measurement  [char:gss]
2A19  Battery Level  [char:gss]
2A1A  Battery Power State  [char:gss]
2A1B  Battery Level State  [char:gss]
2A1C  Temperature Measurement  [char:gss]
2A1D  Temperature Type  [char:gss]
2A1E  Intermediate Temperature  [char:gss]
2A1F  Temperature Celsius  [char:gss]
2A20  Temperature Fahrenheit  [char:gss]
2A21  Measurement Interval  [char:gss]
2A22  Boot Keyboard Input Report  [char:gss]
2A23  System ID  [char:gss]
2A24  Model Number String  [char:gss]
2A25  Serial Number String  [char:gss]
2A26  Firmware Revision String  [char:gss]
2A27  Hardware Revision String  [char:gss]
2A28  Software Revision String  [char:gss]
2A29  Manufacturer Name String  [char:gss]
2A2A  IEEE 11073-20601 Regulatory Certification Data List  [char:gss]
2A2B  Current Time  [char:gss]
2A2C  Magnetic Declination  [char:gss]
2A2F  Position 2D  [char:gss]
2A30  Position 3D  [char:gss]
2A31  Scan Refresh  [char:gss]
2A32  Boot Keyboard Output Report  [char:gss]
2A33  Boot Mouse Input Report  [char:gss]
2A34  Glucose Measurement Context  [char:gss]
2A35  Blood Pressure Measurement  [char:gss]
2A36  Intermediate Cuff Pressure  [char:gss]
2A37  Heart Rate Measurement  [char:gss]
2A38  Body Sensor Location  [char:gss]
2A39  Heart Rate Control Point  [char:gss]
2A3A  Removable  [char:gss]
2A3B  Service Required  [char:gss]
2A3C  Scientific Temperature Celsius  [char:gss]
2A3D  String  [char:gss]
2A3E  Network Availability  [char:gss]
2A3F  Alert Status  [char:gss]
2A40  Ringer Control point  [char:gss]
2A41  Ringer Setting  [char:gss]
2A42  Alert Category ID Bit Mask  [char:gss]
2A43  Alert Category ID  [char:gss]
2A44  Alert Notification Control Point  [char:gss]
2A45  Unread Alert Status  [char:gss]
2A46  New Alert  [char:gss]
2A47  Supported New Alert Category  [char:gss]
2A48  Supported Unread Alert Category  [char:gss]
2A49  Blood Pressure Feature  [char:gss]
2A4A  HID Information  [char:gss]
2A4B  Report Map  [char:gss]
2A4C  HID Control Point  [char:gss]
2A4D  Report  [char:gss]
2A4E  Protocol Mode  [char:gss]
2A4F  Scan Interval Window  [char:gss]
2A50  PnP ID  [char:gss]
2A51  Glucose Feature  [char:gss]
2A52  Record Access Control Point  [char:gss]
2A53  RSC Measurement  [char:gss]
2A54  RSC Feature  [char:gss]
2A55  SC Control Point  [char:gss]
2A56  Digital  [char:gss]
2A57  Digital Output  [char:gss]
2A58  Analog  [char:gss]
2A59  Analog Output  [char:gss]
2A5A  Aggregate  [char:gss]
2A5B  CSC Measurement  [char:gss]
2A5C  CSC Feature  [char:gss]
2A5D  Sensor Location  [char:gss]
2A5E  PLX Spot-Check Measurement  [char:gss]
2A5F  PLX Continuous Measurement Characteristic  [char:gss]
2A60  PLX Features  [char:gss]
2A62  Pulse Oximetry Control Point  [char:gss]
2A63  Cycling Power Measurement  [char:gss]
2A64  Cycling Power Vector  [char:gss]
2A65  Cycling Power Feature  [char:gss]
2A66  Cycling Power Control Point  [char:gss]
2A67  Location and Speed Characteristic  [char:gss]
2A68  Navigation  [char:gss]
2A69  Position Quality  [char:gss]
2A6A  LN Feature  [char:gss]
2A6B  LN Control Point  [char:gss]
2A6C  Elevation  [char:gss]
2A6D  Pressure  [char:gss]
2A6E  Temperature  [char:gss]
2A6F  Humidity  [char:gss]
2A70  True Wind Speed  [char:gss]
2A71  True Wind Direction  [char:gss]
2A72  Apparent Wind Speed  [char:gss]
2A73  Apparent Wind Direction  [char:gss]
2A74  Gust Factor  [char:gss]
2A75  Pollen Concentration  [char:gss]
2A76  UV Index  [char:gss]
2A77  Irradiance  [char:gss]
2A78  Rainfall  [char:gss]
2A79  Wind Chill  [char:gss]
2A7A  Heat Index  [char:gss]
2A7B  Dew Point  [char:gss]
2A7D  Descriptor Value Changed  [char:gss]
2A7E  Aerobic Heart Rate Lower Limit  [char:gss]
2A7F  Aerobic Threshold  [char:gss]
2A80  Age  [char:gss]
2A81  Anaerobic Heart Rate Lower Limit  [char:gss]
2A82  Anaerobic Heart Rate Upper Limit  [char:gss]
2A83  Anaerobic Threshold  [char:gss]
2A84  Aerobic Heart Rate Upper Limit  [char:gss]
2A85  Date of Birth  [char:gss]
2A86  Date of Threshold Assessment  [char:gss]
2A87  Email Address  [char:gss]
2A88  Fat Burn Heart Rate Lower Limit  [char:gss]
2A89  Fat Burn Heart Rate Upper Limit  [char:gss]
2A8A  First Name  [char:gss]
2A8B  Five Zone Heart Rate Limits  [char:gss]
2A8C  Gender  [char:gss]
2A8D  Heart Rate Max  [char:gss]
2A8E  Height  [char:gss]
2A8F  Hip Circumference  [char:gss]
2A90  Last Name  [char:gss]
2A91  Maximum Recommended Heart Rate  [char:gss]
2A92  Resting Heart Rate  [char:gss]
2A93  Sport Type for Aerobic and Anaerobic Thresholds  [char:gss]
2A94  Three Zone Heart Rate Limits  [char:gss]
2A95  Two Zone Heart Rate Limit  [char:gss]
2A96  VO2 Max  [char:gss]
2A97  Waist Circumference  [char:gss]
2A98  Weight  [char:gss]
2A99  Database Change Increment  [char:gss]
2A9A  User Index  [char:gss]
2A9B  Body Composition Feature  [char:gss]
2A9C  Body Composition Measurement  [char:gss]
2A9D  Weight Measurement  [char:gss]
2A9E  Weight Scale Feature  [char:gss]
2A9F  User Control Point  [char:gss]
2AA0  Magnetic Flux Density - 2D  [char:gss]
2AA1  Magnetic Flux Density - 3D  [char:gss]
2AA2  Language  [char:gss]
2AA3  Barometric Pressure Trend  [char:gss]
2AA4  Bond Management Control Point  [char:gss]
2AA5  Bond Management Features  [char:gss]
2AA6  Central Address Resolution  [char:gss]
2AA7  CGM Measurement  [char:gss]
2AA8  CGM Feature  [char:gss]
2AA9  CGM Status  [char:gss]
2AAA  CGM Session Start Time  [char:gss]
2AAB  CGM Session Run Time  [char:gss]
2AAC  CGM Specific Ops Control Point  [char:gss]
2AAD  Indoor Positioning Configuration  [char:gss]
2AAE  Latitude  [char:gss]
2AAF  Longitude  [char:gss]
2AB0  Local North Coordinate  [char:gss]
2AB1  Local East Coordinate  [char:gss]
2AB2  Floor Number  [char:gss]
2AB3  Altitude  [char:gss]
2AB4  Uncertainty  [char:gss]
2AB5  Location Name  [char:gss]
2AB6  URI  [char:gss]
2AB7  HTTP Headers  [char:gss]
2AB8  HTTP Status Code  [char:gss]
2AB9  HTTP Entity Body  [char:gss]
2ABA  HTTP Control Point  [char:gss]
2ABB  HTTPS Security  [char:gss]
2ABC  TDS Control Point  [char:gss]
2ABD  OTS Feature  [char:gss]
2ABE  Object Name  [char:gss]
2ABF  Object Type  [char:gss]
2AC0  Object Size  [char:gss]
2AC1  Object First-Created  [char:gss]
2AC2  Object Last-Modified  [char:gss]
2AC3  Object ID  [char:gss]
2AC4  Object Properties  [char:gss]
2AC5  Object Action Control Point  [char:gss]
2AC6  Object List Control Point  [char:gss]
2AC7  Object List Filter  [char:gss]
2AC8  Object Changed  [char:gss]
2AC9  Resolvable Private Address Only  [char:gss]
2ACC  Fitness Machine Feature  [char:gss]
2ACD  Treadmill Data  [char:gss]
2ACE  Cross Trainer Data  [char:gss]
2ACF  Step Climber Data  [char:gss]
2AD0  Stair Climber Data  [char:gss]
2AD1  Rower Data  [char:gss]
2AD2  Indoor Bike Data  [char:gss]
2AD3  Training Status  [char:gss]
2AD4  Supported Speed Range  [char:gss]
2AD5  Supported Inclination Range  [char:gss]
2AD6  Supported Resistance Level Range  [char:gss]
2AD7  Supported Heart Rate Range  [char:gss]
2AD8  Supported Power Range  [char:gss]
2AD9  Fitness Machine Control Point  [char:gss]
2ADA  Fitness Machine Status  [char:gss]
2ADB  Mesh Provisioning Data In  [char:gss]
2ADC  Mesh Provisioning Data Out  [char:gss]
2ADD  Mesh Proxy Data In  [char:gss]
2ADE  Mesh Proxy Data Out  [char:gss]
2AE0  Average Current  [char:gss]
2AE1  Average Voltage  [char:gss]
2AE2  Boolean  [char:gss]
2AE3  Chromatic Distance From Planckian  [char:gss]
2AE4  Chromaticity Coordinates  [char:gss]
2AE5  Chromaticity In CCT And Duv Values  [char:gss]
2AE6  Chromaticity Tolerance  [char:gss]
2AE7  CIE 13.3-1995 Color Rendering Index  [char:gss]
2AE8  Coefficient  [char:gss]
2AE9  Correlated Color Temperature  [char:gss]
2AEA  Count 16  [char:gss]
2AEB  Count 24  [char:gss]
2AEC  Country Code  [char:gss]
2AED  Date UTC  [char:gss]
2AEE  Electric Current  [char:gss]
2AEF  Electric Current Range  [char:gss]
2AF0  Electric Current Specification  [char:gss]
2AF1  Electric Current Statistics  [char:gss]
2AF2  Energy  [char:gss]
2AF3  Energy In A Period Of Day  [char:gss]
2AF4  Event Statistics  [char:gss]
2AF5  Fixed String 16  [char:gss]
2AF6  Fixed String 24  [char:gss]
2AF7  Fixed String 36  [char:gss]
2AF8  Fixed String 8  [char:gss]
2AF9  Generic Level  [char:gss]
2AFA  Global Trade Item Number  [char:gss]
2AFB  Illuminance  [char:gss]
2AFC  Luminous Efficacy  [char:gss]
2AFD  Luminous Energy  [char:gss]
2AFE  Luminous Exposure  [char:gss]
2AFF  Luminous Flux  [char:gss]
2B00  Luminous Flux Range  [char:gss]
2B01  Luminous Intensity  [char:gss]
2B02  B02 Mass Flow  [char:gss]
2B03  Perceived Lightness  [char:gss]
2B04  Percentage 8  [char:gss]
2B05  Power  [char:gss]
2B06  Power Specification  [char:gss]
2B07  Relative Runtime In A Current Range  [char:gss]
2B08  Relative Runtime In A Generic Level Range  [char:gss]
2B09  Relative Value In A Voltage Range  [char:gss]
2B0A  Relative Value In An Illuminance Range  [char:gss]
2B0B  Relative Value In A Period Of Day  [char:gss]
2B0C  Relative Value In A Temperature Range  [char:gss]
2B0D  Temperature 8  [char:gss]
2B0E  Temperature 8 In A Period Of Day  [char:gss]
2B0F  Temperature 8 Statistics  [char:gss]
2B10  Temperature Range  [char:gss]
2B11  Temperature Statistics  [char:gss]
2B12  Time Decihour 8  [char:gss]
2B13  Time Exponential 8  [char:gss]
2B14  Time Hour 24  [char:gss]
2B15  Time Millisecond 24  [char:gss]
2B16  Time Second 16  [char:gss]
2B17  Time Second 8  [char:gss]
2B18  Voltage  [char:gss]
2B19  Voltage Specification  [char:gss]
2B1A  Voltage Statistics  [char:gss]
2B1B  Volume Flow  [char:gss]
2B1C  Chromaticity Coordinate  [char:gss]
2B1D  RC Feature  [char:gss]
2B1D  RC Feature  [char:gss]
2B1E  RC Settings  [char:gss]
2B1E  RC Settings  [char:gss]
2B1F  Reconnection Configuration Control Point  [char:gss]
2B1F  Reconnection Configuration Control Point  [char:gss]
2B20  IDD Status Changed  [char:gss]
2B20  IDD Status Changed  [char:gss]
2B21  IDD Status  [char:gss]
2B21  IDD Status  [char:gss]
2B22  IDD Annunciation Status  [char:gss]
2B22  IDD Annunciation Status  [char:gss]
2B23  IDD Features  [char:gss]
2B23  IDD Features  [char:gss]
2B24  IDD Status Reader Control Point  [char:gss]
2B24  IDD Status Reader Control Point  [char:gss]
2B25  IDD Command Control Point  [char:gss]
2B25  IDD Command Control Point  [char:gss]
2B26  IDD Command Data  [char:gss]
2B26  IDD Command Data  [char:gss]
2B27  IDD Record Access Control Point  [char:gss]
2B27  IDD Record Access Control Point  [char:gss]
2B28  IDD History Data  [char:gss]
2B28  IDD History Data  [char:gss]
2B29  Client Supported Features  [char:gss]
2B2A  Database Hash  [char:gss]
2B2B  BSS Control Point  [char:gss]
2B2C  BSS Response  [char:gss]
2B2D  Emergency ID  [char:gss]
2B2E  Emergency Text  [char:gss]
2B34  Enhanced Blood Pressure Measurement  [char:gss]
2B35  Enhanced Intermediate Cuff Pressure  [char:gss]
2B36  Blood Pressure Record  [char:gss]
2B38  BR-EDR Handover Data  [char:gss]
2B39  Bluetooth SIG Data  [char:gss]
2B3A  Server Supported Features  [char:gss]
2B3B  Physical Activity Monitor Features  [char:gss]
2B3C  General Activity Instantaneous Data  [char:gss]
2B3D  General Activity Summary Data  [char:gss]
2B3E  CardioRespiratory Activity Instantaneous Data  [char:gss]
2B3F  CardioRespiratory Activity Summary Data  [char:gss]
2B40  Step Counter Activity Summary Data  [char:gss]
2B41  Sleep Activity Instantaneous Data  [char:gss]
2B42  Sleep Activity Summary Data  [char:gss]
2B43  Physical Activity Monitor Control Point  [char:gss]
2B44  Activity Current Session  [char:gss]
2B45  Physical Activity Session Descriptor  [char:gss]
2B46  Preferred Units  [char:gss]
2B47  High Resolution Height  [char:gss]
2B48  Middle Name  [char:gss]
2B49  Stride Length  [char:gss]
2B4A  Handedness  [char:gss]
2B4B  Device Wearing Position  [char:gss]
2B4C  Four Zone Heart Rate Limits  [char:gss]
2B4D  High Intensity Exercise Threshold  [char:gss]
2B4E  Activity Goal  [char:gss]
2B4F  Sedentary Interval Notification  [char:gss]
2B50  Caloric Intake  [char:gss]
2B51  TMAP Role  [char:gss]
2B77  Audio Input State  [char:gss]
2B78  Gain Settings Attribute  [char:gss]
2B79  Audio Input Type  [char:gss]
2B7A  Audio Input Status  [char:gss]
2B7B  Audio Input Control Point  [char:gss]
2B7C  Audio Input Description  [char:gss]
2B7D  Volume State  [char:gss]
2B7E  Volume Control Point  [char:gss]
2B7F  Volume Flags  [char:gss]
2B80  Volume Offset State  [char:gss]
2B81  Audio Location  [char:gss]
2B82  Volume Offset Control Point  [char:gss]
2B83  Audio Output Description  [char:gss]
2B84  Set Identity Resolving Key  [char:gss]
2B85  Coordinated Set Size  [char:gss]
2B86  Set Member Lock  [char:gss]
2B87  Set Member Rank  [char:gss]
2B8C  Carbon Dioxide Concentration  [char:gss]
2B8E  Device Time Feature  [char:gss]
2B8F  Device Time Parameters  [char:gss]
2B90  Device Time  [char:gss]
2B91  Device Time Control Point  [char:gss]
2B92  Time Change Log Data  [char:gss]
2B93  Media Player Name  [char:gss]
2B94  Media Player Icon Object ID  [char:gss]
2B95  Media Player Icon URL  [char:gss]
2B96  Track Changed  [char:gss]
2B97  Track Title  [char:gss]
2B98  Track Duration  [char:gss]
2B99  Track Position  [char:gss]
2B9A  Playback Speed  [char:gss]
2B9B  Seeking Speed  [char:gss]
2B9C  Current Track Segments Object ID  [char:gss]
2B9D  Current Track Object ID  [char:gss]
2B9E  Next Track Object ID  [char:gss]
2B9F  Parent Group Object ID  [char:gss]
2BA0  Current Group Object ID  [char:gss]
2BA1  Playing Order  [char:gss]
2BA2  Playing Orders Supported  [char:gss]
2BA3  Media State  [char:gss]
2BA4  Media Control Point  [char:gss]
2BA5  Media Control Point Opcodes Supported  [char:gss]
2BA6  Search Results Object ID  [char:gss]
2BA7  Search Control Point  [char:gss]
2BA9  Media Player Icon Object Type  [char:gss]
2BAA  Track Segments Object Type  [char:gss]
2BAB  Track Object Type  [char:gss]
2BAC  Group Object Type  [char:gss]
2BAD  Constant Tone Extension Enable  [char:gss]
2BAE  Advertising Constant Tone Extension Minimum Length  [char:gss]
2BAF  Advertising Constant Tone Extension Minimum Transmit Count  [char:gss]
2BB0  Advertising Constant Tone Extension Transmit Duration  [char:gss]
2BB1  Advertising Constant Tone Extension Interval  [char:gss]
2BB2  Advertising Constant Tone Extension PHY  [char:gss]
2BB3  Bearer Provider Name  [char:gss]
2BB4  Bearer UCI  [char:gss]
2BB5  Bearer Technology  [char:gss]
2BB6  Bearer URI Schemes Supported List  [char:gss]
2BB7  Bearer Signal Strength  [char:gss]
2BB8  Bearer Signal Strength Reporting Interval  [char:gss]
2BB9  Bearer List Current Calls  [char:gss]
2BBA  Content Control ID  [char:gss]
2BBB  Status Flags  [char:gss]
2BBC  Incoming Call Target Bearer URI  [char:gss]
2BBD  Call State  [char:gss]
2BBE  Call Control Point  [char:gss]
2BBF  Call Control Point Optional Opcodes  [char:gss]
2BC0  Termination Reason  [char:gss]
2BC1  Incoming Call  [char:gss]
2BC2  Call Friendly Name  [char:gss]
2BC3  Mute  [char:gss]
2BC4  Sink ASE  [char:gss]
2BC5  Source ASE  [char:gss]
2BC6  ASE Control Point  [char:gss]
2BC7  Broadcast Audio Scan Control Point  [char:gss]
2BC8  Broadcast Receive State  [char:gss]
2BC9  Sink PAC  [char:gss]
2BCA  Sink Audio Locations  [char:gss]
2BCB  Source PAC  [char:gss]
2BCC  Source Audio Locations  [char:gss]
2BCD  Available Audio Contexts  [char:gss]
2BCE  Supported Audio Contexts  [char:gss]
2BCF  Ammonia Concentration  [char:gss]
2BD0  Carbon Monoxide Concentration  [char:gss]
2BD1  Methane Concentration  [char:gss]
2BD2  Nitrogen Dioxide Concentration  [char:gss]
2BD3  Non-Methane Volatile Organic Compounds Concentration  [char:gss]
2BD4  Ozone Concentration  [char:gss]
2BD5  Particulate Matter - PM1 Concentration  [char:gss]
2BD6  Particulate Matter - PM2.5 Concentration  [char:gss]
2BD7  Particulate Matter - PM10 Concentration  [char:gss]
2BD8  Sulfur Dioxide Concentration  [char:gss]
2BD9  Sulfur Hexafluoride Concentration  [char:gss]
2BDA  Hearing Aid Features  [char:gss]
2BDB  Hearing Aid Preset Control Point  [char:gss]
2BDC  Active Preset Index  [char:gss]
2BDD  Stored Health Observations  [char:gss]
2BDE  Fixed String 64  [char:gss]
2BDF  High Temperature  [char:gss]
2BE0  High Voltage  [char:gss]
2BE1  Light Distribution  [char:gss]
2BE2  Light Output  [char:gss]
2BE3  Light Source Type  [char:gss]
2BE4  Noise  [char:gss]
2BE5  Relative Runtime in a Correlated Color Temperature Range  [char:gss]
2BE6  Time Second 32  [char:gss]
2BE7  VOC Concentration  [char:gss]
2BE8  Voltage Frequency  [char:gss]
2BE9  Battery Critical Status  [char:gss]
2BEA  Battery Health Status  [char:gss]
2BEB  Battery Health Information  [char:gss]
2BEC  Battery Information  [char:gss]
2BED  Battery Level Status  [char:gss]
2BEE  Battery Time Status  [char:gss]
2BEF  Estimated Service Date  [char:gss]
2BF0  Battery Energy Status  [char:gss]
2BF1  Observation Schedule Changed  [char:gss]
2BF2  Current Elapsed Time  [char:gss]
2BF3  Health Sensor Features  [char:gss]
2BF4  GHS Control Point  [char:gss]
2BF5  LE GATT Security Levels  [char:gss]
2BF6  ESL Address  [char:gss]
2BF7  AP Sync Key Material  [char:gss]
2BF8  ESL Response Key Material  [char:gss]
2BF9  ESL Current Absolute Time  [char:gss]
2BFA  ESL Display Information  [char:gss]
2BFB  ESL Image Information  [char:gss]
2BFC  ESL Sensor Information  [char:gss]
2BFD  ESL LED Information  [char:gss]
2BFE  ESL Control Point  [char:gss]
2BFF  UDI for Medical Devices  [char:gss]
2C00  GMAP Role  [char:gss]
2C01  UGG Features  [char:gss]
2C02  UGT Features  [char:gss]
2C03  BGS Features  [char:gss]
2C04  BGR Features  [char:gss]
2C05  Percentage 8 Steps  [char:gss]
2F7CABCE-808D-411F-9A0C-BB92BA96C102  Apple Entity Update  [char:apple]
398168AA-0111-4EC0-B1FA-171671270608  Helium Hotspot WiFi Connect  [char:helium]
506A55C4-B5E7-46FA-8326-8ACAEB1189EB  Sensor Hub Temperature  [char:nordic]
51838AFF-2D9A-B32A-B32A-8187E41664BA  Sensor Hub Pressure  [char:nordic]
54220001-F6A5-4007-A371-722F4EBD8436  MDS Supported Features Characteristic  [char:memfault]
54220002-F6A5-4007-A371-722F4EBD8436  MDS Device Identifier Characteristic  [char:memfault]
54220003-F6A5-4007-A371-722F4EBD8436  MDS Device Data URI Characteristic  [char:memfault]
54220004-F6A5-4007-A371-722F4EBD8436  MDS Device Authorization Characteristic  [char:memfault]
54220005-F6A5-4007-A371-722F4EBD8436  MDS Device Data Export Characteristic  [char:memfault]
57A70001-9350-11ED-A1EB-0242AC120002  Status Characteristic  [char:nordic]
69D1D8F3-45E1-49A8-9821-9BBDFDAAD9D9  Apple Control Point  [char:apple]
6A9A7A8E-FCA5-4B02-AAB2-54C531665872  Sensor Hub VOC  [char:nordic]
6E400002-B5A3-F393-E0A9-E50E24DCCA9E  UART RX Characteristic  [char:nordic]
6E400003-B5A3-F393-E0A9-E50E24DCCA9E  UART TX Characteristic  [char:nordic]
753E3050-DF06-4B53-B090-5E1D810C4383  Sensor Hub Humidity  [char:nordic]
7731DE63-BC6A-4100-8AB1-89B2356B038B  Helium Hotspot WiFi SSID  [char:helium]
7DFC6001-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6002-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6003-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6004-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6005-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6101-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6102-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6103-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6104-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6105-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6106-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6107-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6108-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6201-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6202-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC6203-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7004-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7005-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7006-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7007-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7008-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7009-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC700A-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC700B-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC700C-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7103-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7104-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7105-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7106-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7107-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7108-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC7109-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC710B-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC710C-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC710D-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC8003-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC8004-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
7DFC9001-7D1C-4951-86AA-8D9728F8D66C  Apple Reserved Characteristic  [char:apple]
82754BBB-6ED3-4D69-A0E1-F19F6B654EC2  Sensor Hub Red Color  [char:nordic]
8CC6E0B3-98C5-40CC-B1D8-692940E6994B  Helium Hotspot WiFi Remove  [char:helium]
8E400001-F315-4F60-9FB8-838830DAEA50  Experimental Buttonless DFU  [char:nordic]
8EC90001-F315-4F60-9FB8-838830DAEA50  DFU Control Point  [char:nordic]
8EC90002-F315-4F60-9FB8-838830DAEA50  DFU Packet  [char:nordic]
8EC90003-F315-4F60-9FB8-838830DAEA50  Buttonless DFU Without Bonds  [char:nordic]
8EC90004-F315-4F60-9FB8-838830DAEA50  Buttonless DFU With Bonds  [char:nordic]
932C32BD-0002-47A2-835A-A8D455B859DD  Philips Hue Light On/Off Toggle  [char:philips-hue]
932C32BD-0003-47A2-835A-A8D455B859DD  Philips Hue Light Brightness Level  [char:philips-hue]
932C32BD-0005-47A2-835A-A8D455B859DD  Philips Hue Light Color  [char:philips-hue]
9B3C81D8-57B1-4A8A-B8DF-0E56F7CA51C2  Apple Remote Command  [char:apple]
9C4314F2-8A0C-45FD-A58D-D4A7E64C3A57  Helium Hotspot WiFi MAC Address  [char:helium]
9FBF120D-6301-42D9-8C58-25E699A21DBD  Apple Notification Source  [char:apple]
A3C87501-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone Capabilities  [char:google]
A3C87502-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone Active Slot  [char:google]
A3C87503-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone Advertising Interval  [char:google]
A3C87504-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone Radio Tx Power  [char:google]
A3C87505-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone (Advanced) Advertised Tx Power  [char:google]
A3C87506-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone Lock State  [char:google]
A3C87507-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone Unlock  [char:google]
A3C87508-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone Public ECDH Key  [char:google]
A3C87509-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone EID Identity Key  [char:google]
A3C8750A-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone ADV Slot Data  [char:google]
A3C8750B-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone Advanced Factory Reset  [char:google]
A3C8750C-8ED3-4BDF-8A39-A01BEBEDE295  Eddystone (Advanced) Remain Connectable  [char:google]
AD79CBCE-65DF-4BC6-BDD4-8CE2B6B75C59  Sensor Hub IAQ  [char:nordic]
ADAF0001-C332-42A8-93BD-25E905756CB8  Adafruit Sensor Measurement Period  [char:adafruit]
ADAF0002-C332-42A8-93BD-25E905756CB8  Adafruit Sensor Service Version  [char:adafruit]
ADAF0100-4669-6C65-5472-616E73666572  Adafruit Version  [char:adafruit]
ADAF0101-C332-42A8-93BD-25E905756CB8  Adafruit Temperature  [char:adafruit]
ADAF0200-4669-6C65-5472-616E73666572  Adafruit Raw TX/RX  [char:adafruit]
ADAF0201-C332-42A8-93BD-25E905756CB8  Adafruit Acceleration  [char:adafruit]
ADAF0301-C332-42A8-93BD-25E905756CB8  Adafruit Light Level  [char:adafruit]
ADAF0401-C332-42A8-93BD-25E905756CB8  Adafruit Gyro  [char:adafruit]
ADAF0501-C332-42A8-93BD-25E905756CB8  Adafruit Magnetic  [char:adafruit]
ADAF0601-C332-42A8-93BD-25E905756CB8  Adafruit Pressed  [char:adafruit]
ADAF0701-C332-42A8-93BD-25E905756CB8  Adafruit Humidity  [char:adafruit]
ADAF0801-C332-42A8-93BD-25E905756CB8  Adafruit Pressure  [char:adafruit]
ADAF0901-C332-42A8-93BD-25E905756CB8  Adafruit Pixel Pin  [char:adafruit]
ADAF0902-C332-42A8-93BD-25E905756CB8  Adafruit Pixel Pin Type  [char:adafruit]
ADAF0903-C332-42A8-93BD-25E905756CB8  Adafruit Pixel Data  [char:adafruit]
ADAF0904-C332-42A8-93BD-25E905756CB8  Adafruit Pixel Buffer Size  [char:adafruit]
ADAF0A01-C332-42A8-93BD-25E905756CB8  Adafruit Color  [char:adafruit]
ADAF0B01-C332-42A8-93BD-25E905756CB8  Adafruit Sound Samples  [char:adafruit]
ADAF0B02-C332-42A8-93BD-25E905756CB8  Adafruit Number of Channels  [char:adafruit]
ADAF0C01-C332-42A8-93BD-25E905756CB8  Adafruit Tone  [char:adafruit]
ADAF0D01-C332-42A8-93BD-25E905756CB8  Adafruit Quaternions  [char:adafruit]
ADAF0D02-C332-42A8-93BD-25E905756CB8  Adafruit Calibration In  [char:adafruit]
ADAF0D03-C332-42A8-93BD-25E905756CB8  Adafruit Calibration Out  [char:adafruit]
ADAF0E01-C332-42A8-93BD-25E905756CB8  Adafruit Proximity  [char:adafruit]
B833D34F-D871-422C-BF9E-8E6EC117D57E  Helium Hotspot Diagnostics  [char:helium]
C0953A6D-1004-48C2-B382-A947F4A0A673  Sensor Hub CO2  [char:nordic]
C6B2F38C-23AB-46D8-A6AB-A3A870BBD5D7  Apple Entity Attribute  [char:apple]
D083B2BD-BE16-4600-B397-61512CA2F5AD  Helium Hotspot Onboarding Key  [char:helium]
D435F5DE-01A4-4E7D-84BA-DFD347F60275  Helium Hotspot Assert Location  [char:helium]
D7515033-7E7B-45BE-803F-C8737B171A29  Helium Hotspot WiFi Services  [char:helium]
DA2E7828-FBCE-4E01-AE9E-261174997C48  SMP Characteristic  [char:apache]
DB7F9F36-92CE-4509-A2EF-AF72BA38FB48  Sensor Hub Green Color  [char:nordic]
DF3B16CA-C985-4DA2-A6D2-9B9B9ABDB858  Helium Hotspot Add Gateway  [char:helium]
E125BDA4-6FB8-11EA-BC55-0242AC130003  Helium Hotspot WiFi Configured Services  [char:helium]
E2A00002-EC31-4EC3-A97A-1C34D87E9878  Edge Impulse Remote Management RX Characteristic  [char:nordic]
E2A00003-EC31-4EC3-A97A-1C34D87E9878  Edge Impulse Remote Management TX Characteristic  [char:nordic]
E5866BD6-0288-4476-98CA-EF7DA6B4D289  Helium Hotspot Ethernet Online  [char:helium]
E95D0D2D-251D-470A-A062-FA1922DFA9A8  micro:bit Scrolling Delay  [char:microbit]
E95D1B25-251D-470A-A062-FA1922DFA9A8  micro:bit Temperature Period  [char:microbit]
E95D23C4-251D-470A-A062-FA1922DFA9A8  micro:bit Client Requirements  [char:microbit]
E95D386C-251D-470A-A062-FA1922DFA9A8  micro:bit Magnetometer Period  [char:microbit]
E95D5404-251D-470A-A062-FA1922DFA9A8  micro:bit Client Event  [char:microbit]
E95D5899-251D-470A-A062-FA1922DFA9A8  micro:bit Pin AD Configuration  [char:microbit]
E95D7B77-251D-470A-A062-FA1922DFA9A8  micro:bit LED Matrix State  [char:microbit]
E95D8D00-251D-470A-A062-FA1922DFA9A8  micro:bit Pin Data  [char:microbit]
E95D9250-251D-470A-A062-FA1922DFA9A8  micro:bit Temperature  [char:microbit]
E95D93B1-251D-470A-A062-FA1922DFA9A8  micro:bit DFU Control  [char:microbit]
E95D93EE-251D-470A-A062-FA1922DFA9A8  micro:bit LED Text  [char:microbit]
E95D9715-251D-470A-A062-FA1922DFA9A8  micro:bit Magnetometer Bearing  [char:microbit]
E95D9775-251D-470A-A062-FA1922DFA9A8  micro:bit Event  [char:microbit]
E95DB84C-251D-470A-A062-FA1922DFA9A8  micro:bit Requirements  [char:microbit]
E95DB9FE-251D-470A-A062-FA1922DFA9A8  micro:bit Pin I/O Configuration  [char:microbit]
E95DCA4B-251D-470A-A062-FA1922DFA9A8  micro:bit Accelerometer Data  [char:microbit]
E95DD822-251D-470A-A062-FA1922DFA9A8  micro:bit PWM Control  [char:microbit]
E95DDA90-251D-470A-A062-FA1922DFA9A8  micro:bit Button A State  [char:microbit]
E95DDA91-251D-470A-A062-FA1922DFA9A8  micro:bit Button B State  [char:microbit]
E95DFB11-251D-470A-A062-FA1922DFA9A8  micro:bit Magnetometer Data  [char:microbit]
E95DFB24-251D-470A-A062-FA1922DFA9A8  micro:bit Accelerometer Period  [char:microbit]
EF680101-9B35-4933-9B10-52FFA9740042  Thingy Device Name  [char:nordic]
EF680102-9B35-4933-9B10-52FFA9740042  Thingy Advertising Parameters  [char:nordic]
EF680104-9B35-4933-9B10-52FFA9740042  Thingy Connection Parameters  [char:nordic]
EF680105-9B35-4933-9B10-52FFA9740042  Thingy Eddystone URL  [char:nordic]
EF680106-9B35-4933-9B10-52FFA9740042  Thingy Cloud Token  [char:nordic]
EF680107-9B35-4933-9B10-52FFA9740042  Thingy FW Version  [char:nordic]
EF680108-9B35-4933-9B10-52FFA9740042  Thingy MTU Request  [char:nordic]
EF680201-9B35-4933-9B10-52FFA9740042  Thingy Temperature  [char:nordic]
EF680202-9B35-4933-9B10-52FFA9740042  Thingy Pressure  [char:nordic]
EF680203-9B35-4933-9B10-52FFA9740042  Thingy Humidity  [char:nordic]
EF680204-9B35-4933-9B10-52FFA9740042  Thingy Air Quality  [char:nordic]
EF680205-9B35-4933-9B10-52FFA9740042  Thingy Color  [char:nordic]
EF680206-9B35-4933-9B10-52FFA9740042  Thingy Configuration  [char:nordic]
EF680301-9B35-4933-9B10-52FFA9740042  Thingy LED State  [char:nordic]
EF680302-9B35-4933-9B10-52FFA9740042  Thingy Button State  [char:nordic]
EF680303-9B35-4933-9B10-52FFA9740042  Thingy EXT Pin  [char:nordic]
EF680401-9B35-4933-9B10-52FFA9740042  Thingy Motion Config  [char:nordic]
EF680402-9B35-4933-9B10-52FFA9740042  Thingy Tap  [char:nordic]
EF680403-9B35-4933-9B10-52FFA9740042  Thingy Orientation  [char:nordic]
EF680404-9B35-4933-9B10-52FFA9740042  Thingy Quaternion  [char:nordic]
EF680405-9B35-4933-9B10-52FFA9740042  Thingy Pedometer  [char:nordic]
EF680406-9B35-4933-9B10-52FFA9740042  Thingy Raw Data  [char:nordic]
EF680407-9B35-4933-9B10-52FFA9740042  Thingy Euler  [char:nordic]
EF680408-9B35-4933-9B10-52FFA9740042  Thingy Rotation Matrix  [char:nordic]
EF680409-9B35-4933-9B10-52FFA9740042  Thingy Heading  [char:nordic]
EF68040A-9B35-4933-9B10-52FFA9740042  Thingy Gravity Vector  [char:nordic]
EF680501-9B35-4933-9B10-52FFA9740042  Thingy Sound Config  [char:nordic]
EF680502-9B35-4933-9B10-52FFA9740042  Thingy Speaker Data  [char:nordic]
EF680503-9B35-4933-9B10-52FFA9740042  Thingy Speaker Status  [char:nordic]
EF680504-9B35-4933-9B10-52FFA9740042  Thingy Microphone  [char:nordic]
F000FFC1-0451-4000-B000-000000000000  Texas Instruments Image Identify  [char:ti]
F000FFC2-0451-4000-B000-000000000000  Texas Instruments Image Block  [char:ti]
F000FFC5-0451-4000-B000-000000000000  Texas Instruments OAD Control  [char:ti]
F5D2EAB5-41E8-4F7C-AEF7-C9FFF4C544C0  Sensor Hub Blue Color  [char:nordic]
FA3CF070-D0C7-4668-96C4-86125C8AC5DF  Sensor Hub Battery  [char:nordic]
FE2C1233-8366-4814-8EB0-01DE32100BEA  Fast Pair Model ID  [char:google]
FE2C1234-8366-4814-8EB0-01DE32100BEA  Fast Pair Key-based Pairing  [char:google]
FE2C1235-8366-4814-8EB0-01DE32100BEA  Fast Pair Passkey  [char:google]
FE2C1236-8366-4814-8EB0-01DE32100BEA  Fast Pair Account Key  [char:google]
FE2C1237-8366-4814-8EB0-01DE32100BEA  Fast Pair Data  [char:google]
6E400002-B5A3-F393-E0A9-E50E24DCCA9E  Nordic UART RX Characteristic  [vendor-128]
6E400003-B5A3-F393-E0A9-E50E24DCCA9E  Nordic UART TX Characteristic  [vendor-128]
8EC90003-F315-4F60-9FB8-838830DAEA50  Nordic DFU Buttonless Char  [vendor-128]
00001531-1212-EFDE-1523-785FEABCD123  Nordic Legacy DFU Control Point  [vendor-128]
9FBF120D-6301-42D9-8C58-25E699A21DBD  ANCS Notification Source  [vendor-128]
69D1D8F3-45E1-49A8-9821-9BBDFDAAD9D9  ANCS Control Point  [vendor-128]
22EAC6E9-24D6-4BB5-BE44-B36ACE7C7BFB  ANCS Data Source  [vendor-128]
9B3C81D8-57B1-4A8A-B8DF-0E56F7CA51C2  AMS Remote Command  [vendor-128]
2F7CABCE-808D-411F-9A0C-BB92BA96C102  AMS Entity Update  [vendor-128]
C6B2F38C-23AB-46D8-A6AB-A3A870BBD5D7  AMS Entity Attribute  [vendor-128]
8667556C-9A37-4C91-84ED-54EE27D90049  Apple Continuity Char  [vendor-128]
AF0BADB1-5B99-43CD-917A-A77BC549E3CC  Apple Nearby Char  [vendor-128]
0000FFE1-0000-1000-8000-00805F9B34FB  HM-10 / TI Serial Char  [vendor-128]
0000FFF1-0000-1000-8000-00805F9B34FB  Serial RX (FFF1)  [vendor-128]
0000FFF2-0000-1000-8000-00805F9B34FB  Serial TX (FFF2)  [vendor-128]
F000FFC1-0451-4000-B000-000000000000  TI OAD Image Identify  [vendor-128]
F000FFC2-0451-4000-B000-000000000000  TI OAD Image Block  [vendor-128]
